IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2025-02-14T16:16:53"
Preprocessor: "IfcOpenShell 0.8.1-c49ca69"
Originating system: "IfcOpenShell 0.8.1-c49ca69"
Application: "12d Model" version "15.0C1n" identifier "12d Model" by Organization "BG&E Pty Ltd" description "BG&E Pty Ltd"
Application: "12d Model" version "15.0C1n" identifier "12d Model" by Organization "BG&E Pty Ltd" description "BG&E Pty Ltd"
Application: "Bonsai" version "0.8.1-alpha250208-3832077" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

People and organizations
  2 x Person "Pravin.Muthukrishnan" of Organization "BG&E Pty Ltd" description "BG&E Pty Ltd"
  2 x Owner history of Person "Pravin.Muthukrishnan" of Organization "BG&E Pty Ltd" description "BG&E Pty Ltd" | application "12d Model" version "15.0C1n" identifier "12d Model" by Organization "BG&E Pty Ltd" description "BG&E Pty Ltd" | change NOCHANGE | created 1739508662 (2025-02-14T04:51:02Z)
  2 x Owner history of Person "Pravin.Muthukrishnan" of Organization "BG&E Pty Ltd" description "BG&E Pty Ltd" | application "12d Model" version "15.0C1n" identifier "12d Model" by Organization "BG&E Pty Ltd" description "BG&E Pty Ltd" | change MODIFIED | created 1739508662 (2025-02-14T04:51:02Z) | last modified 1739510213 (2025-02-14T05:16:53Z) by Person "Pravin.Muthukrishnan" of Organization "BG&E Pty Ltd" description "BG&E Pty Ltd" with "Bonsai" version "0.8.1-alpha250208-3832077" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "DRAINAGE DESIGN" | description "No description set"
  IFCSITE "Default Site" | description "Description of Default Site"
    contains 1 element
      1 x IFCFLOWSEGMENT | object type "EXISTING (RETAINED)" | names: "5" | descriptions: "5-1 to 1-1" | property sets: 12d Model

Property sets
  12d Model | properties | on 1 object (1 IFCFLOWSEGMENT)
    Geometry: Justification = "Invert" (IFCLABEL); Start x = 289080.818499209 (IFCREAL); Start y = 5822851.36621952 (IFCREAL); Start z = 118.736 (IFCREAL); End x = 289081.570466963 (IFCREAL); End y = 5822857.54453541 (IFCREAL); End z = 118.736 (IFCREAL)
    Pipe Name = "5-1 to 1-1" (IFCLABEL)
    Pipe Type = "EXISTING (RETAINED)" (IFCLABEL)
    calculated critical cover chainage = 2.24873590275508 (IFCREAL)
    calculated design cover = 1.1 (IFCREAL)
    calculated design drop = 0.02 (IFCREAL)
    calculated design grade minimum = 1. (IFCREAL)
    calculated direct pipe flow total major = 0. (IFCREAL)
    calculated direct pipe flow total minor = 0. (IFCREAL)
    calculated direct pit and pipe flow total major = 0. (IFCREAL)
    calculated direct pit and pipe flow total minor = 0. (IFCREAL)
    calculated drop = 0. (IFCREAL)
    calculated ds deflection = 89.4496469263205 (IFCREAL)
    calculated hgl ds = 118.736 (IFCREAL)
    calculated hgl us = 118.736 (IFCREAL)
    calculated invert ds = 118.736 (IFCREAL)
    calculated invert us = 118.736 (IFCREAL)
    calculated pipe grade 1 in = 1000000. (IFCREAL)
    calculated pipe grade = -0. (IFCREAL)
    calculated pipe length = 7.19890895752825 (IFCREAL)
    calculated pipe vert angle = 0. (IFCREAL)
    calculated pipe vert ds deflection angle = -4.09980829540645 (IFCREAL)
    calculated us deflection = 0. (IFCREAL)
    colour = "orange" (IFCLABEL)
    conduit shape = "Circular" (IFCLABEL)
    critical barrel = 0 (IFCINTEGER)
    critical side = 0 (IFCINTEGER)
    diameter = 0.3 (IFCREAL)
    invert ds = 118.736 (IFCREAL)
    invert us = 118.736 (IFCREAL)
    lock ds il = 1 (IFCINTEGER)
    lock us il = 1 (IFCINTEGER)
    lplot: name = "EX" (IFCLABEL)
    minimum cover = 1.67561504823626 (IFCREAL)
    nominal diameter = 0.3 (IFCREAL)
    nominal pipe size = "300" (IFCLABEL)
    pipe colour = 8 (IFCINTEGER)
    pipe id = 35 (IFCINTEGER)
    pipe name = "5-1 to 1-1" (IFCLABEL)
    pipe sched: group = "EX" (IFCLABEL)
    pipe size = "300" (IFCLABEL)
    pipe type = "EXISTING (RETAINED)" (IFCLABEL)
    roughness text = "n=0.013" (IFCLABEL)