IFC building model
Schema: "IFC4"
File name: "building_service_element_air-terminal.ifc"
Time stamp: "2011-11-11T23:58:37"
Preprocessor: "Constructivity 0.9.1"
Originating system: "Constructivity 0.9.1"
Application: "Constructivity" version "0.9.1" identifier "CONSTRUCTIVITY" by Organization "Constructivity.com LLC"

People and organizations
  Person id "Tim" of Organization "Tim-PC"
  Owner history of Person id "Tim" of Organization "Tim-PC" | application "Constructivity" version "0.9.1" identifier "CONSTRUCTIVITY" by Organization "Constructivity.com LLC" | state READWRITE | change NOTDEFINED | created 1321055806 (2011-11-11T23:56:46Z)

Units
  LENGTHUNIT: inch (conversion based)

Spatial structure
IFCPROJECT "Project"
  IFCBUILDING
    contains 2 elements
      1 x IFCAIRTERMINAL | type IFCAIRTERMINALTYPE "Acme Diffuser 1234"
      1 x IFCDUCTSEGMENT | FLEXIBLESEGMENT | names: "Duct Segment #1" | material: profiles "Duct Segment" ("Body": "Aluminum")

Types
  IFCAIRTERMINALTYPE "Acme Diffuser 1234" | DIFFUSER | 1 occurrence | property sets: Pset_AirTerminalTypeCommon, Pset_ManufacturerTypeInformation | description "Ceiling diffuser"

Property sets
  Pset_DistributionPortCommon | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ColorCode (no value)
    PortNumber (no value)
  Pset_DistributionPortTypeAirConditioning | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionSubType (no value)
    ConnectionType in {"OUTSIDESLEEVE"} (IFCLABEL)
    DryBulbTemperature =  .. 
    NominalHeight = 12. (IFCPOSITIVELENGTHMEASURE) [inch (conversion based)]
    NominalWidth = 12. (IFCPOSITIVELENGTHMEASURE) [inch (conversion based)]
    Pressure =  .. 
    Velocity =  .. 
    VolumetricFlowRate =  .. 
    WetBulbTemperature =  .. 
  Pset_AirTerminalTypeCommon | properties | on 1 type object
    AirDiffusionPerformanceIndex (no value)
    AirFlowrateRange =  .. 
    AirFlowrateVersusFlowControlElement (ifcpropertytablevalue)
    CoreSetHorizontal (no value)
    CoreSetVertical (no value)
    CoreType in {}
    DischargeDirection in {}
    EffectiveArea (no value)
    FaceType in {}
    FinishColor (no value)
    FinishType in {}
    FlowControlType in {}
    FlowPattern in {}
    HasIntegralControl (no value)
    HasSoundAttenuator (no value)
    HasThermalInsulation (no value)
    MountingType in {}
    NeckArea (no value)
    NumberOfSlots (no value)
    Reference (no value)
    Shape in {"SQUARE"} (IFCLABEL)
    SlotLength (no value)
    SlotWidth (no value)
    Status in {}
    TemperatureRange =  .. 
    ThrowLength (no value)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber (no value)
    AssemblyPlace in {"FACTORY"} (IFCLABEL)
    GlobalTradeItemNumber (no value)
    Manufacturer = "Acme" (IFCLABEL)
    ModelLabel = "Ceiling Diffuser" (IFCLABEL)
    ModelReference = "1234" (IFCLABEL)
    ProductionYear = "2011" (IFCLABEL)