IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
File name: "building_element_configuration_wall.ifc"
Time stamp: "2011-12-12T22:18:35"
Author: "Architect"
Organization: "Test Office"
Preprocessor: "IFC Engine DLL version 1.03 beta"
Originating system: "Geometry example"
Authorization: "The authorising person"
Application: "Test Application" version "0.10" identifier "TA 1001" by Organization "RDF" description "RDF Ltd."

People and organizations
  Person "Peter" "Bonsma" of Organization "RDF" description "RDF Ltd."
  Owner history of Person "Peter" "Bonsma" of Organization "RDF" description "RDF Ltd." | application "Test Application" version "0.10" identifier "TA 1001" by Organization "RDF" description "RDF Ltd." | change NOTDEFINED | created 1323724715 (2011-12-12T21:18:35Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Default Project" | description "Description of Default Project"
  IFCSITE "Default Site" | latitude 24° 28′ 0″ | longitude 54° 25′ 0″ | elevation above sea level 10. | description "Description of Default Site"
    IFCBUILDING "Default Building" | postal address: "RDF Ltd.", "Main Office", "32", "Bankya", "Sofia", "1320", "Bulgaria" | description "Description of Default Building"
      IFCBUILDINGSTOREY "Default Building Storey" | elevation 0. | description "Description of Default Building Storey"
        contains 2 elements
          1 x IFCWALLSTANDARDCASE | names: "Wall for Test Example" | descriptions: "Description of Wall" | material: layers ("Name of the material used for the wall" 300.) | property sets: Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Window for Test Example" | WINDOW | SINGLE_PANEL | names: "Window for Test Example" | descriptions: "Description of Window" | material: constituents "Constituent Set for Window" ("Framing": "Glass", "Framing": "Wood") | property sets: Pset_WindowCommon

Types
  IFCWINDOWTYPE "Window for Test Example" | WINDOW | SINGLE_PANEL | 1 occurrence | description "Description of Window Type"

Property sets
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 2.4E-1 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 7.E-1 (IFCPOSITIVERATIOMEASURE)
    Infiltration = 3.E-1 (IFCVOLUMETRICFLOWRATEMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    SecurityRating = "" (IFCLABEL)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 2.4E-1 (IFCTHERMALTRANSMITTANCEMEASURE)